Renault Koleos II (Phase II) 2.0 Blue dCi (190 Hp) 4x4-i X-Tronic 2019, 2020, 2021, 2022, 2023, 2024 Specs

General information

Brand Renault

Model Koleos

Generation Koleos II (Phase II)

Modification (Engine) 2.0 Blue dCi (190 Hp) 4x4-i X-Tronic

Start of production April, 2019 year

Powertrain Architecture Internal Combustion engine

Body type SUV

Seats 5

Doors 5

Performance specs

Combined fuel consumption (WLTP) 6.9-7.1 l/100 km

34.09 - 33.13 US mpg

40.94 - 39.79 UK mpg

14.49 - 14.08 km/l

CO2 emissions (WLTP) 181-184 g/km

CO2 emissions 150 g/km

Fuel Type Diesel

Acceleration 0 - 100 km/h 10.1 sec

Acceleration 0 - 62 mph 10.1 sec

Acceleration 0 - 60 mph (Calculated by Auto-Data.net) 9.6 sec

Maximum speed 198 km/h

123.03 mph

Emission standard Euro 6 d-TEMP

Weight-to-power ratio 9.3 kg/Hp, 107.3 Hp/tonne

Weight-to-torque ratio 4.7 kg/Nm, 214.7 Nm/tonne

Engine specs

Power 190 Hp @ 3500 rpm.

Power per litre 95.2 Hp/l

Torque 380 Nm @ 1750 rpm.

280.27 lb.-ft. @ 1750 rpm.

Engine layout Front, Transverse

Engine Model/Code M9R 730

Engine displacement 1995 cm3

121.74 cu. in.

Number of cylinders 4

Engine configuration Inline

Cylinder Bore 84 mm

3.31 in.

Piston Stroke 88 mm

3.46 in.

Number of valves per cylinder 4

Fuel injection system Diesel Commonrail

Engine aspiration Turbocharger, Intercooler

Engine oil capacity 7.6 l

8.03 US qt | 6.69 UK qt

Engine oil specification Log in to see.

Coolant 7.9 l

8.35 US qt | 6.95 UK qt

Engine systems Particulate filter

Space, Volume and weights

Kerb Weight 1770 kg

3902.18 lbs.

Max. weight 2309 kg

5090.47 lbs.

Max load 539 kg

1188.29 lbs.

Trunk (boot) space - minimum 498 l

17.59 cu. ft.

Trunk (boot) space - maximum 1706 l

60.25 cu. ft.

Fuel tank capacity 60 l

15.85 US gal | 13.2 UK gal

AdBlue tank 16 l

4.23 US gal | 3.52 UK gal

Dimensions

Length 4673 mm

183.98 in.

Width 1813 mm

71.38 in.

Width including mirrors 2063 mm

81.22 in.

Height 1667 mm

65.63 in.

Wheelbase 2705 mm

106.5 in.

Front track 1591 mm

62.64 in.

Rear (Back) track 1586 mm

62.44 in.

Front overhang 929 mm

36.57 in.

Rear overhang 1039 mm

40.91 in.

Ride height (ground clearance) 189 mm

7.44 in.

Minimum turning circle (turning diameter) 11.4 m

37.4 ft.

Approach angle 18.4°

Departure angle 24.7°

Drivetrain, brakes and suspension specs

Drive wheel All wheel drive (4x4)

Number of gears and type of gearbox automatic transmission X-Tronic

Front suspension Independent type McPherson

Rear suspension Independent multi-link suspension

Front brakes Ventilated discs, 320 mm

Rear brakes Disc, 292 mm

Assisting systems ABS (Anti-lock braking system)

Steering type Steering rack and pinion

Tires size 225/65 R17 102H; 225/60 R18 100H; 225/55 R19 99V

Wheel rims size 17; 18; 19